|  |  |
| --- | --- |
|  | **Dreadnought Clay Roof Tiles**  **Tel: 01384 77405**  [www.dreadnought-tiles.co.uk](http://www.nbsplus.co.uk/process.asp?DreadnoughtTiles)  office@dreadnought-tiles.co.uk |

To complete the clause, select the appropriate wording from below. Highlighted text can be ‘dragged and dropped’ to save typing.

**H60 PLAIN ROOF TILING**

**700 DRY VENTILATED RIDGES:**

**Dreadnought Tileline Dry Fix Ridge Systems.**A dry ventilated ridge system using 300 mm long half round ridge tiles in a smoothfaced or sandfaced finish.  The natural burnt clay colours are produced entirely by control of the kiln atmosphere and without the use of colouring agents.  These colours are permanent and unaffected by exposure to UHV light.   
All products comply with BS EN 1304.  
The ridge tiles are laid on top of ventilated filler units and ridge connectors and clamped by 50 mm wide fixing plates, nailed through the apex of the ridge connectors into the timber ridge batten. Galvanised ridge batten straps are used to fix the ridge batten to the rafters to provide the required ventilation air space at the ridge.  
Ventilation: 5,000 mm2 per linear metre.  
The roof pitch must be quoted when ordering.  
Consult with Dreadnought Tiles technical literature for details. Hinton, Perry & Davenhill Ltd can also provide a design and specification service and it is recommended that they are consulted early in the design process.

**Dry ridge fixing battens:** Not applicable.

**Dry ridge tiles:  
Manufacturer:** Hinton, Perry & Davenhill Ltd, Dreadnought Works, Pensnett, Brierley Hill, West Midlands, DY5 4TH. Tel: 01384 77405. Fax: 01384 74553. Email: [office@dreadnought-tiles.co.uk](mailto:office@dreadnought-tiles.co.uk) Web: [www.dreadnought-tiles.co.uk](http://www.nbsplus.co.uk/process.asp?DreadnoughtTiles)   
**Product reference:** Dreadnought Tileline Dry Fix Ridge System Ref: RVDP.  
**Ridge tiles:** Dreadnought Clay Plain Half Round Ridge Tiles Ref: RVD, HR.  
**Colour:**   
To match roof tiles.  
Sandfaced finishes:  
Red Sandfaced / Brown Heather Sandfaced / Red-Blue Blend Sandfaced / Brown Antique Sandfaced / Staffs Blue Sandfaced / Dark Heather Sandfaced  
Smoothfaced finishes:  
Red Smoothfaced / Plum Red Smoothfaced / Brown Brindle Smoothfaced /  Red-Blue Blend Smoothfaced / Brown Antique Smoothfaced / Blue Brindle Smoothfaced / Staffs Blue Smoothfaced  
**Pitch:** 35° / 40° / 45° / 50°  
Standard pitches. Consult with Dreadnought for availability of alternatives.