|  |  |
| --- | --- |
|  | **Dreadnought Clay Roof Tiles** **Tel: 01384 77405**[www.dreadnought-tiles.co.uk](http://www.nbsplus.co.uk/process.asp?DreadnoughtTiles)office@dreadnought-tiles.co.uk  |

To complete the clause, select the appropriate wording from below. Highlighted text can be ‘dragged and dropped’ to save typing.

**H60 PLAIN ROOF TILING**

**850 ROOF SLOPE TERMINALS:**

**Clay Clad Tileline Tile Vent.**A ventilator tile in a smoothfaced or sandfaced finish. The natural burnt clay colours are produced entirely by control of the kiln atmosphere and without the use of colouring agents. These colours are permanent and unaffected by exposure to UHV light.
All products comply with BS EN 1304
A pipe adapter and flexible connection pipe is available for soil venting or mechanical extraction.
Tile dimensions: 495 mm long x 320 mm deep, equal to 3 roof tiles.
Ventilation: 7500 mm2 per ventilator tile.
Pipe adapter spigot: suits 100 mm, 125 mm or 150 mm pipes.
Not designed for the extraction of hot combustible gases. The ventilator must be sited at least 900 mm from any opening into the roof.
The roof pitch must be quoted when ordering.
Consult with Dreadnought Tiles technical literature for details. Hinton, Perry & Davenhill Ltd can also provide a design and specification service and it is recommended that they are consulted early in the design process.

**Ventilator tiles:
Manufacturer:** Hinton, Perry & Davenhill Ltd, Dreadnought Works, Pensnett, Brierley Hill, West Midlands, DY5 4TH. Tel: 01384 77405. Fax: 01384 74553. Email: office@dreadnought-tiles.co.uk Web: [www.dreadnought-tiles.co.uk](http://www.nbsplus.co.uk/process.asp?DreadnoughtTiles)
**Product reference:** Dreadnought Tileline Tile Vent, complete with Tileline Adapter and Flexible Pipe.
**Colour:**To match roof tiles.
Sandfaced finishes:
Red Sandfaced / Brown Heather Sandfaced / Red-Blue Blend Sandfaced / Brown Antique Sandfaced / Staffs Blue Sandfaced / Dark Heather Sandfaced
Smoothfaced finishes:
Red Smoothfaced / Plum Red Smoothfaced / Brown Brindle Smoothfaced /  Red-Blue Blend Smoothfaced / Brown Antique Smoothfaced / Blue Brindle Smoothfaced / Staffs Blue Smoothfaced
**Pitch:** 35° / 40° / 45° / 50°
Standard pitches. Consult with Dreadnought for availability of alternatives.